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PRE-BID CONFERENCE AGENDA
Durango SFU
Paving and Drainline
PROJECT # S25WAQ-9789
DQ1 – 2026*405

April 15, 2026 @ 11 AM

Taylor Halford – Project Manager
Cell Phone (720) 666-8072
Email taylor.halford@state.co.us

Nathanael Bokelman – Project Manager			Connor Young – Design Engineer
Office Phone (970) 375-6719 					Office Phone (303) 291-7397 	
Cell Phone (970) 903-1549					Cell Phone (804) 432-2560
E-mail	nathanael.bokelman@state.co.us			E-mail connor.young@state.co.us

1. Bidding Information:

· All questions shall be in writing and sent to Connor Young at connor.young@state.co.us (only questions in writing via email will be answered).
· Any Addendums will be posted on the State VSS website www.colorado.gov/VSS
· All addendums must be acknowledged on the bid proposal. It is the bidder’s responsibility to check for addendums. Failure to acknowledge may result in rejection of bid. 
· Bids will be accepted up to the due date/time. All bids shall be to the attention of Connor Young.
· Bonding – bonding, including bid bond, is required if a bid is over   $150,000.00.
· Pre-bid Attendance List will be posted on the State VSS website. 

2. Proposed Project Timing:

· Questions will be allowed until 5PM on April 17. 2026. Any questions will be addressed in a Final Addendum that will be posted to the State VSS website by 5 pm on April 23, 2026, if not sooner.
· Bids Due on May 5, 2026 by 11:00 am – email to connor.young@state.co.us.(bids are preferred to be received electronically by email, but mailed or hand-delivered bids will be accepted. If mailed or hand-delivered, please ensure to label “Attn: Connor Young”). Any bids, electronic or physical, received after the deadline will not be accepted.
· Notification and the Bid Tabulation will be sent to all Bidders as promptly as possible following the bid opening. The lowest responsible bidder will then be contacted and issued a Notice of Intent to Award as long as the bid falls within the Project’s budget and the bidder meets the required qualifications.
· Notice to Proceed – It is expected that a PO or Contract will take 2-4 weeks to be processed once all required documents (insurance certificate, W-9, etc.) are received from the Awarded Contractor.  Notice to Proceed is anticipated to be issued by early August. Mid-August – Early September is the best window for construction for the hatchery.

3. General Information:

· All quantities are estimates only and may be increased or decreased as needed and allowed per the General Conditions for Construction.
· Please pay close attention to ALL project drawings and specifications. 
· No permits are anticipated with this project.
· Any contractor working within the city limits of Durango must have a Durango Business License. Please refer to https://www.durangoco.gov/177/Business-Licensing for more information.
· All work shall be contained within CPW’s property.
· Construction will only be allowed between 7am and sunset on week days (unless written approval obtained from Project Manager). No construction on weekends and holidays.
· Expected Construction Start = August 17, 2026 (tentative). The goal is to be completed by the end of September at the latest. 
· Construction schedule coordination is important on this project to ensure that construction does not negatively impact hatchery operations.
4. Site Work

· Contractor shall perform or hire out utility location services to located any existing utilities in the project area.
· Contractor shall dig a trench from the upper inlet down past the existing bend in the pipe. Contractor shall remove and dispose of (off property) existing storm infrastructure within that trench
· Contractor shall remove and dispose of all existing asphalt outside of trench area and within the area shown on the drawings. All existing concrete pads shall remain.
· Contractor shall install new PVC to HDPE adapter, new bend, and new slotted drain pipe system (ADS Duraslot or approved equal) at the same location as the existing pipe system. Elevations shall match drawings. The slotted drain pipe system also will have concrete “encasement” as shown on the drawings and details.
· If a product other than ADS Duraslot is requested/desired, the contractor must get approval at the time of written questions/final addendum. If not, and the contractor receives approval for a different product afterwards, the contractor must honor the bid-listed price of the installation of that approved product/system, including all components, connections, etc.
· Contractor shall install new asphalt – matching grades along the drainage system and tying into existing grades around the perimeter of asphalt area. Grades shall not be flatter than 0.5% if possible.
· If budget allows, optional bid items will be included with this project. This includes replacing the existing PVC from the new adapter to the existing inlet by the entrance, concrete encasing the new stretch of pipe for cover protection, installing new underground roof drain pipes from the existing roof drains to the new slotted drain pipe system. Any combination of these items can be selected to achieve the maximum amount of work received at the lowest bid price.
Questions?
· 
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